# MidiCC Node

The MidiCC node outputs controller values filtered by MIDI channel and control number.

Select the channel from the menu on the left. To set a control number, right click on the right menu to set the value manually.

The valid range of control numbers is between 1 and 127 inclusive. Some MIDI devices allow you to specify a control number, but standard control numbers are as follows:

- 1 Modulation wheel
- 7 Volume
- 10 Pan
- 11 Expression
- 64 Sustain pedal
- 91 Reverb level
- 92 Tremolo level
- 93 Chorus level
- 94 Celeste level
- 95 Phaser level
- 121 All controllers off
- 123 All notes off